#!/bin/sh
#
#	mkboot 2.0 - make boot floppy, make root device bootable, etc.
#							Author: Kees J. Bot

trap 'e=$?; rm -f /tmp/mkb.$$; exit $e' 0 2

mdec=/usr/mdec	# bootstraps

# Check arguments.
case "$#:$1" in
1:bootable | 1:hdboot | [12]:fdboot )
	action=$1 dev=$2 size=$3
	;;
*)	echo "Usage: $0 [bootable | hdboot | fdboot [device]]" >&2
	exit 1
esac

# Get the device table.
. /etc/fstab

# The real root device may be the RAM disk.
realroot=`printroot -r`

# If it's an initial fstab, pretend root is real root
if [ $root = "/dev/ROOT" ]
then	root=$realroot
fi

case $action in
bootable | hdboot)
	# We need the root device.

	if [ $realroot = $root ]
	then
		rootdir=
	else
		umount $root 2>/dev/null
		mount $root /mnt || exit
		rootdir=/mnt
	fi
esac

case $action in
bootable)
	# Install the boot monitor on the root device and make it bootable.
	install -cs -m 644 $mdec/boot $rootdir/boot/boot || exit
	sync
	installboot -device $root $mdec/bootblock /boot/boot || exit
	test $realroot != $root && umount $root
	;;
hdboot)
	# Install a new image on the root device.
	if [ ! -d $rootdir/boot/image ]
	then
		 /boot/image is not yet a directory!  Fix it.
		su root -c \
		    "exec mv $rootdir/boot/image /M"
		install -d $rootdir/boot/image
		su root -c \
		    "exec mv $rootdir/M $rootdir/boot/image/`uname -r`.`uname -v`"
	fi

	sh tell_config OS_RELEASE . OS_VERSION >/tmp/mkb.$$
	version=`sed 's/[" 	]//g;/^$/d' </tmp/mkb.$$`

	revision=`cat revision 2>/dev/null`

	if [ -z "$revision" ]
	then	rrevision=""
	else	rrevision=r$revision
	fi

	oldrev=$revision

	target="${version}r${revision}"

	if [ -z "$revision" ]
	then
		revision=0
		rrevision=""
	elif [ -f $rootdir/boot/image/$target ]
	then
		if [ $rootdir/boot/image/$target -newer image ]
		then
			echo "$root:/boot/image/$target is up to date"
			test $realroot != $root && umount $root
			exit 0
		fi
		revision=`expr $revision + 1`
		rrevision=r$revision
	fi
	target="${version}${rrevision}"

	set -- `ls -t $rootdir/boot/image`

	case $# in
	0|1|2|3)
		# Not much there, do not remove a thing.
		;;
	*)
		# Remove the third-newest image in /boot/image, but
		# only if there's an older one (which is kept). 
		echo "rm $root:/boot/image/$3"
		rm -f "$rootdir/boot/image/$3"
	esac

	# Install the new image.
	echo "install image $root:/boot/image/$target"
	install -o root -m 600 image $rootdir/boot/image/$target || exit

	# Save the revision number.
	test "$revision" != "$oldrev" && echo $revision >revision

	test $realroot != $root && umount $root
	echo "Done."
	;;
fdboot)
	# fdboot: Make a boot floppy.

	if [ -z "$dev" ]
	then
		echo -n \
"Finish the name of the floppy device to write (by default 'fd0'): /dev/";
		read dev
		case "$dev" in
		'')	dev=/dev/fd0
			;;
		/dev/*)
			;;
		*)	dev=/dev/$dev
		esac
	fi

	# Make a file system.
	umount $dev 2>/dev/null
	if mkfs -B 1024 -i 512 $dev
	then	:
	else
		echo "mkfs of $dev failed."
		exit 1;
	fi

	# Install /dev, /boot/boot and /boot/image.
	mount $dev /mnt || exit
	mkdir -p /mnt/boot/image || exit
	cpdir /dev /mnt/dev || exit
	cp -p $mdec/boot /mnt/boot/boot || exit
	cp -p image /mnt/boot/image/ || exit
	umount $dev || exit

	# Make bootable and copy the boot parameters.
	installboot -d $dev $mdec/bootblock /boot/boot || exit
	pfile=fdbootparams
	if [ -f $pfile ]
	then	echo "Using floppy boot parameters from file $pfile."
		edparams $dev "`cat $pfile`" || exit
	else	echo "Copying floppy boot parameters from $root."
		dd if=$root of=$dev skip=1 seek=1 count=1 conv=silent || exit
	fi
	edparams $dev 'main(){delay 2000;boot}; save' || exit
	echo "Test kernel installed on $dev"
	;;
esac
sync
exit 0
